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	Certificate of Competence
Hand Back Engineer Levels 1 to 4
	TEF 3306
Issue 1 December 2022



Carry out inspection to confirm the line is fit for operational use.
Carry out inspection to raise / remove a speed restriction

	Name:
	
	Certificate No.
	

	Job Title:
	
	Date of Certification:
	

	Is competent to confirm the line is fit for operational use and to raise/remove speed restrictions as detailed below:
(Initial boxes to indicate competence, strike through the other boxes)

	Scope of Activity
(see NR/L3/TRK/1020, Table 7 for additional detail)
	Minimum Competency
	Authority Level

	
	
	Level 1
	Level 2
	Level 3
	Level 4

	
	
	Up to any line speed
	Up to 60mph
	Between 65 and 90mph
	Up to any line speed

	1
	Preparatory / follow up works
and
the work does not affect the operational infrastructure

	Person in Charge/Team leader/ Checker
	
	
	
	

	2
	Engineering work
and
the work does not affect track geometry

	TR11 or TR13
	
	
	
	

	3
	Engineering work undertaken with a line blockage
and
the work is undertaken manually and
does affect or restore track geometry

	TR11 or TR13
	
	
	
	

	4
	Engineering work, undertaken with a line blockage, using one of the following on-track machines:
· Tamper;
· S&C tamper;
where the track is handed back at the current line speed or ‘trackwork’ ESR / TSR
	TR05 or TR13
	
	
	
	

	
	•	Ballast Regulator
	TR05 or TR13
	
	
	
	

	
	

	5
	Remove 20mph ESR imposed for track defect:
(including, but not limited to)
· rail defect / broken rail
· broken fishplate
· temporary joint
· adjustment switch support
· rough ride
	TR11 or TR13
	
	
	
	



	6
	After completion of mechanised maintenance work or refurbishment work:
confirm track is fit for operational use to:
· hand back track at current/planned line speed
OR
· remove ‘trackwork’ TSR.
	TR12 or TR13
	
	
	
	

	7
	After completion of renewal work:
confirm track is fit for operational use to:
· hand back track at current/planned line speed
OR
· remove ‘trackwork’ TSR
	TR13
	
	
	
	

	*
	Undertaken Absolute Track Geometry Training for Enhanced Permissible Speed Routes (NR/L3/TRK/0030)
	ATG
	
	
	
	

	Completion of this form:
This form should be completed, or updated, following completion of training, mentoring and assessment.
“C” denotes competent to carry out activity. “M” denotes if competent to Mentor activity. 

	Endorsements and comments:
This section can be used to exclude certain asset types from the authority to work (e.g. S&C) or record dates/details of training/mentoring.










	[bookmark: _Hlk104976525]I have assessed and confirm Hand Back Engineer as competent to undertake the role. CRE(Track) 
	Signed:
Print Name:
	Date:

	I agree I am competent to undertake the required role and understand my responsibilities. (Hand Back Engineer)
	Signed:
Print Name:
	Date:

	I accept the Hand Back Engineer as being suitable for the project / programme of works (CEM)
	Signed:
Print Name:
	Date:

	Notes:
· Additional rows can be added to add further clarity to accepted activities
· Activity consideration/limitations:
· Activity 1 and 2 - Work includes use of On Track Plant or not
· All activities- On Plain Line or S&C track
· Understanding that further compliance checks might be required by other non-track disciplines (5.4)
· The Hand Back Engineer shall be independently assessed- not appointing themselves (5.6)
· Review capability at least every 2 years (5.5)



Certificate for use in line with NR/L3/TRK/1020 and track competencies (Tr11, Tr12 & Tr13)
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